# Notes on front light module

## Pitfalls

* Uses 4.7V universal module, NOT 3.3 V.
* Headlights are connected in series.
* Eyebrows and indicators are the same LED, therefore some logic is needed to switch between those two.